TURNPACK    D5L6 Site Preparation Sheet — Spectrum Control

MIDAS D5L6
De-Lidder System
Site Preparation & Installation Checklist
Please complete and return this form prior to scheduled installation.
	Customer Information
	

	Company Name:
	Spectrum Control de Mexico

	Contact Name:
	

	Phone / Email:
	

	Installation Address:
	

	Scheduled Install Date:
	

	Turnpack Sales Order #:
	SO2524915

	Customer PO #:
	PO.MX32667



1.  Facility Requirements
	✓
	Requirement
	Specification

	☐
	Machine footprint (W × D × H)
	24″ × 22″ × 14″

	☐
	Recommended clear work area (W × D × H)
	30″ × 24″ × 26″ (room to rotate for rear access)

	☐
	Bench load capacity
	≥ 250 lbs; solid, level, non-vibrating

	☐
	Machine weight
	141 lbs (2-person lift)

	☐
	Tool storage
	6″ shelf minimum; lockable drawer recommended

	☐
	Operating environment
	≤ 40 °C, ≤ 90% RH, non-explosive

	☐
	Location
	In or adjacent to a microelectronics clean room



2.  Electrical Requirements
	✓
	Requirement
	Specification

	☐
	Supply voltage (factory-configured)
	110 V AC, 60 Hz, single phase

	☐
	Current draw
	______ A  (confirm against machine nameplate)

	☐
	Circuit
	Separate from sensitive instrumentation circuits (frequent motor cycles)

	☐
	Connection
	NEMA 5-15 grounded outlet; standard North American cord supplied

	☐
	Outlet location
	Within reach of rear panel

	☐
	Grounding
	ESD wrist-strap connector to single chassis ground point / neutral



Note: This unit is factory-configured for 110 V / 60 Hz service. No transformer or plug adapter is required for standard Mexican facility power (127 V nominal, 60 Hz).
3.  Process Gases, Air & Water
None required. The de-lidder is a dry process — no compressed air, nitrogen, or water is needed.
4.  Vacuum & Particle Control
	✓
	Requirement
	Specification

	☐
	Particle-control vacuum
	Included — self-contained ULPA-filtered unit

	☐
	Connection
	1.5″ ID ESD-conductive hose to machine vacuum outlet

	☐
	Cleanroom central vacuum (optional)
	May connect via 1.5″ conductive outlet in lieu of supplied unit

	☐
	Vent / exhaust
	Not required (ULPA filtration)



5.  Safety & ESD
	✓
	Requirement
	Specification

	☐
	Enclosed cutter with dual lid interlocks
	Standard — cutter stops when lid opens

	☐
	Spindle lock for tool changes
	Provided in tool kit

	☐
	Safety glasses for operators
	Recommended

	☐
	ESD controls per microelectronics practice
	Customer-provided




6.  Pre-Installation Verification
Please confirm the following items are ready before the installation technician arrives:
	✓
	Item
	Ready?

	☐
	Bench in place — ≥ 250 lb capacity, level and non-vibrating
	

	☐
	110 V / 60 Hz outlet within reach of rear panel, separate from instrumentation circuits
	

	☐
	~30″ × 24″ clear work area with room to rotate the machine for rear access
	

	☐
	Space at bench for the particle-control vacuum unit
	

	☐
	ESD ground point available at the bench
	

	☐
	Clear delivery path (machine ships in an export crate; 2-person lift)
	

	☐
	Personnel available for installation and operator training
	

	☐
	Sample devices available for process validation (recommended)
	



7.  Additional Notes / Special Requirements
	Additional Notes / Special Requirements

	

	



8.  Customer Acknowledgment
By signing below, the customer confirms that all site preparation requirements listed above will be completed prior to the scheduled installation date.
	
	

	Customer Signature
	Date

	
	

	Printed Name / Title
	Phone / Email



Questions? Contact your Turnpack representative for assistance with site preparation or installation scheduling.
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